**ECUE\_TR\_BOARD\_PWR\_V1-2**

**Layer STACKUP**

**~ Nickel 5 µm**

**Nickel**

**Top layer, plating**

**~ Copper 17 µm**

**RAW material**

**Copper 17 µm**

**Top layer**

**FR4 800 µm**

**Bottom\_Layer, plating**

**~ Copper 17 µm**

**Copper 17 µm**

**Bottom\_Layer**

**~ Nickel 5 µm**

**Nickel**

**In all the case, the thickness at the level of the PADs must be, at least, 870 µm +/- 90 µm**